Block Write
Time:  11:21:22 - 191ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:22 - 194ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  0.562341332435608
Bytes:  4
Param Data:
0x00, 	0x8F, 	0xF5, 	0x9A



Block Write
Time:  11:21:25 - 151ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:25 - 155ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  0.630957365036011
Bytes:  4
Param Data:
0x00, 	0xA1, 	0x86, 	0x6C



Block Write
Time:  11:21:25 - 680ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:25 - 683ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  0.707945764064789
Bytes:  4
Param Data:
0x00, 	0xB5, 	0x3B, 	0xEF



Block Write
Time:  11:21:26 - 120ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:26 - 124ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  0.794328212738037
Bytes:  4
Param Data:
0x00, 	0xCB, 	0x59, 	0x18



Block Write
Time:  11:21:26 - 559ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:26 - 561ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  0.891250908374786
Bytes:  4
Param Data:
0x00, 	0xE4, 	0x29, 	0x05



Block Write
Time:  11:21:27 - 064ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:27 - 067ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  1
Bytes:  4
Param Data:
0x01, 	0x00, 	0x00, 	0x00



Block Write
Time:  11:21:27 - 383ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:27 - 388ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  1.12201845645905
Bytes:  4
Param Data:
0x01, 	0x1F, 	0x3C, 	0x9A



Block Write
Time:  11:21:27 - 817ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:27 - 827ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  1.25892543792725
Bytes:  4
Param Data:
0x01, 	0x42, 	0x48, 	0xF0



Block Write
Time:  11:21:28 - 305ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:28 - 313ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  1.41253751516342
Bytes:  4
Param Data:
0x01, 	0x69, 	0x9C, 	0x0F



Block Write
Time:  11:21:29 - 127ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:29 - 132ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  1.58489316701889
Bytes:  4
Param Data:
0x01, 	0x95, 	0xBB, 	0x8F



Block Write
Time:  11:21:29 - 823ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1slew_mode
Param Address:  0x2089
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  11:21:29 - 826ms
IC:  IC 1
Cell Name:  Single 1
Param Name:  HWGainADAU145XAlg1target
Param Address:  0x2088
Param Value:  1.77827942371368
Bytes:  4
Param Data:
0x01, 	0xC7, 	0x3D, 	0x52



