Block Write
Time:  12:48:22 - 352ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:22 - 368ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  1.77827942371368
Bytes:  4
Param Data:
0x01, 	0xC7, 	0x3D, 	0x52



Block Write
Time:  12:48:22 - 950ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:22 - 950ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  1.58489316701889
Bytes:  4
Param Data:
0x01, 	0x95, 	0xBB, 	0x8F



Block Write
Time:  12:48:23 - 285ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:23 - 300ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  1.41253751516342
Bytes:  4
Param Data:
0x01, 	0x69, 	0x9C, 	0x0F



Block Write
Time:  12:48:23 - 550ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:23 - 550ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  1.25892543792725
Bytes:  4
Param Data:
0x01, 	0x42, 	0x48, 	0xF0



Block Write
Time:  12:48:23 - 856ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:23 - 871ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  1.12201845645905
Bytes:  4
Param Data:
0x01, 	0x1F, 	0x3C, 	0x9A



Block Write
Time:  12:48:24 - 182ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:24 - 198ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  1
Bytes:  4
Param Data:
0x01, 	0x00, 	0x00, 	0x00



Block Write
Time:  12:48:24 - 526ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:24 - 542ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  0.891250908374786
Bytes:  4
Param Data:
0x00, 	0xE4, 	0x29, 	0x05



Block Write
Time:  12:48:24 - 860ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:24 - 875ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  0.794328212738037
Bytes:  4
Param Data:
0x00, 	0xCB, 	0x59, 	0x18



Block Write
Time:  12:48:25 - 170ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:25 - 170ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  0.707945764064789
Bytes:  4
Param Data:
0x00, 	0xB5, 	0x3B, 	0xEF



Block Write
Time:  12:48:25 - 389ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:25 - 405ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  0.630957365036011
Bytes:  4
Param Data:
0x00, 	0xA1, 	0x86, 	0x6C



Block Write
Time:  12:48:25 - 726ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2slew_mode
Param Address:  0x2086
Param Value:  8330
Bytes:  4
Param Data:
0x00, 	0x00, 	0x20, 	0x8A



Safeload Write
Time:  12:48:25 - 742ms
IC:  IC 1
Cell Name:  Single 1_2
Param Name:  HWGainADAU145XAlg2target
Param Address:  0x2085
Param Value:  0.562341332435608
Bytes:  4
Param Data:
0x00, 	0x8F, 	0xF5, 	0x9A



