Safeload Write
Time:  10:43:42 - 114ms
IC:  IC 1
Cell Name:  Gen Filter1
Param Name:  EQFilterSPS300Alg1B2_1
Param Address:  0x005B
Param Value:  0.238148391246796
Bytes:  4
Param Data:
0x00, 	0x3C, 	0xF7, 	0x4B



Safeload Write
Time:  10:43:42 - 114ms
IC:  IC 1
Cell Name:  Gen Filter1
Param Name:  EQFilterSPS300Alg1B1_1
Param Address:  0x005C
Param Value:  -1.20258349180222
Bytes:  4
Param Data:
0xFE, 	0xCC, 	0x23, 	0x7D



Safeload Write
Time:  10:43:42 - 114ms
IC:  IC 1
Cell Name:  Gen Filter1
Param Name:  EQFilterSPS300Alg1B0_1
Param Address:  0x005D
Param Value:  1.28150016069412
Bytes:  4
Param Data:
0x01, 	0x48, 	0x10, 	0x65



Safeload Write
Time:  10:43:42 - 114ms
IC:  IC 1
Cell Name:  Gen Filter1
Param Name:  EQFilterSPS300Alg1A2_1
Param Address:  0x005E
Param Value:  -0.122128903865814
Bytes:  4
Param Data:
0xFF, 	0xE0, 	0xBC, 	0x29



Safeload Write
Time:  10:43:42 - 114ms
IC:  IC 1
Cell Name:  Gen Filter1
Param Name:  EQFilterSPS300Alg1A1_1
Param Address:  0x005F
Param Value:  0.805063784122467
Bytes:  4
Param Data:
0x00, 	0xCE, 	0x18, 	0xA9



Safeload Write
Time:  10:43:42 - 846ms
IC:  IC 1
Cell Name:  Gen Filter1
Param Name:  EQFilterSPS300Alg1B2_1
Param Address:  0x005B
Param Value:  0.155543327331543
Bytes:  4
Param Data:
0x00, 	0x27, 	0xD1, 	0xB0



Safeload Write
Time:  10:43:42 - 846ms
IC:  IC 1
Cell Name:  Gen Filter1
Param Name:  EQFilterSPS300Alg1B1_1
Param Address:  0x005C
Param Value:  -0.874525368213654
Bytes:  4
Param Data:
0xFF, 	0x20, 	0x1F, 	0x1B



Safeload Write
Time:  10:43:42 - 846ms
IC:  IC 1
Cell Name:  Gen Filter1
Param Name:  EQFilterSPS300Alg1B0_1
Param Address:  0x005D
Param Value:  1
Bytes:  4
Param Data:
0x01, 	0x00, 	0x00, 	0x00



Safeload Write
Time:  10:43:42 - 846ms
IC:  IC 1
Cell Name:  Gen Filter1
Param Name:  EQFilterSPS300Alg1A2_1
Param Address:  0x005E
Param Value:  -0.155543327331543
Bytes:  4
Param Data:
0xFF, 	0xD8, 	0x2E, 	0x50



Safeload Write
Time:  10:43:42 - 846ms
IC:  IC 1
Cell Name:  Gen Filter1
Param Name:  EQFilterSPS300Alg1A1_1
Param Address:  0x005F
Param Value:  0.874525368213654
Bytes:  4
Param Data:
0x00, 	0xDF, 	0xE0, 	0xE5



